{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":13,"n_cols":6,"rows_kept":13,"merged":[[0,0,0,5],[12,0,13,5]],"flags":["formulas_cached_only"]}
["物流公司国际部库内照明灯更换项目报价单"]
["序号","项目","单位","工程量","综合单价","合价"]
[1,"原照明灯拆除","套",{"v":220,"d":"220.00"}]
[2,"LED灯：光源105W,灯头E40，白光6500K,显色指数 >80 发光角度200°防水等级IP40,安装高度10米;无光生物危害，符合中国能效二级标准。（含现场安装及辅材）","套",{"v":220,"d":"220.00"}]
[]
[]
[]
[]
[null,"合计"]
[null,"管理费（%）"]
[null,"税金(%计）"]
[null,"工程总价"]
["备注：1、安装要求：每个灯球均需在钢构檩条硬性固定。2、品牌：开尔"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}