{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["分部分项工程清单与计价表"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"分部分项工程清单与计价表","index":0,"n_rows":58,"n_cols":12,"rows_kept":58,"merged":[[0,0,0,11],[1,0,1,11],[2,0,2,3],[2,4,2,8],[2,9,2,11],[3,0,5,0],[3,1,5,1],[3,2,5,2],[3,3,5,3],[3,4,5,4],[3,5,5,5],[3,6,3,10],[3,11,5,11],[4,6,5,6],[4,7,5,7],[4,8,4,10],[16,0,16,6],[17,0,17,11],[18,0,18,3],[18,4,18,8],[18,9,18,11],[19,0,21,0],[19,1,21,1],[19,2,21,2],[19,3,21,3],[19,4,21,4],[19,5,21,5],[19,6,19,10],[19,11,21,11],[20,6,21,6],[20,7,21,7],[20,8,20,10],[32,0,32,6],[33,0,33,11],[34,0,34,3],[34,4,34,8],[34,9,34,11],[35,0,37,0],[35,1,37,1],[35,2,37,2],[35,3,37,3],[35,4,37,4],[35,5,37,5],[35,6,35,10],[35,11,37,11],[36,6,37,6],[36,7,37,7],[36,8,36,10],[48,0,48,6],[49,0,49,6],[50,0,50,11],[51,0,51,3],[51,4,51,8],[51,9,51,11],[52,0,54,0],[52,1,54,1],[52,2,54,2],[52,3,54,3],[52,4,54,4],[52,5,54,5],[52,6,52,10],[52,11,54,11],[53,6,54,6],[53,7,54,7],[53,8,53,10],[56,0,56,6],[57,0,57,6]],"flags":["formulas_cached_only"]}
[]
["分部分项工程清单与计价表"]
["专业工程名称：杭州萧山国际机场航站楼门禁系统读卡器及门禁锁改造安装工程",{"$nulls":3},"标段：",{"$nulls":4},"第 1 页 共 3 页"]
["序号","项目编码","项目名称","项目特征","计量\n单位","工程量","金额(元)",{"$nulls":4},"备注"]
[{"$nulls":6},"综合单价","合价","其中"]
[{"$nulls":8},"人工费","机械费","暂估价"]
["","","读卡器升级","","","","","","","","",""]
["1",null,"读卡器","配置12键数字键盘K86 接入Axiom门禁系统 安装 调试  具体要求详见招标文件","个",258,"","","","","",""]
["2",null,"读卡器","室外设备、配置12键数字键盘 接入Cardax门禁系统 安装 调试  具体要求详见招标文件","个",3,"","","","","",""]
["3",null,"T1门禁系统升级","具体要求详见招标文件","项",1,"","","","","",""]
["4",null,"门禁发卡软件升级","具体要求详见招标文件","项",1,"","","","","",""]
["","","门禁锁升级","","","","","","","","",""]
["6",null,"双门磁力锁","拉力≥550KGS 支持同时接两个门状态LED指示灯 安装 调试  具体要求详见招标文件","把",96,"","","","","",""]
["7",null,"门夹","厂家配套","个",192,"","","","","",""]
["","","新增门禁及监控点","","","","","","","","",""]
["9",null,"门禁网络控制器","型号：UNC-500 安装 调试 具体要求详见招标文件","块",1,"","","","","",""]
["本页小计",{"$nulls":6},"","","","",""]
["分部分项工程清单与计价表"]
["专业工程名称：杭州萧山国际机场航站楼门禁系统读卡器及门禁锁改造安装工程",{"$nulls":3},"标段：",{"$nulls":4},"第 2 页 共 3 页"]
["序号","项目编码","项目名称","项目特征","计量\n单位","工程量","金额(元)",{"$nulls":4},"备注"]
[{"$nulls":6},"综合单价","合价","其中"]
[{"$nulls":8},"人工费","机械费","暂估价"]
["10",null,"二门控制器","型号：RC-2-I 安装 调试 具体要求详见招标文件","块",2,"","","","","",""]
["11",null,"读卡器","配置12键数字键盘K86  安装 调试  具体要求详见招标文件","个",6,"","","","","",""]
["12",null,"双门磁力锁","拉力≥550KGS 支持同时接两个门状态LED指示灯 安装 调试  具体要求详见招标文件","把",3,"","","","","",""]
["13",null,"门夹","厂家配套 安装 调试 具体要求详见招标文件","个",6,"","","","","",""]
["14",null,"紧急开锁器","安装 调试 具体要求详见招标文件","个",3,"","","","","",""]
["15",null,"模拟半球一体机","≥1/3\" CCD　含支架 安装 调试  具体要求详见招标文件","个",3,"","","","","",""]
["16",null,"视频线","SYV75-5 敷设  具体要求详见招标文件","米",600,"","","","","",""]
["17",null,"电源线","RVV2×1.5 敷设  具体要求详见招标文件","米",600,"","","","","",""]
["18",null,"电源线","RVV4×1.0 敷设  具体要求详见招标文件","米",600,"","","","","",""]
["19",null,"电源线","RVV8×1.0 敷设  具体要求详见招标文件","米",1200,"","","","","",""]
["本页小计",{"$nulls":6},"","","","",""]
["分部分项工程清单与计价表"]
["专业工程名称：杭州萧山国际机场航站楼门禁系统读卡器及门禁锁改造安装工程",{"$nulls":3},"标段：",{"$nulls":4},"第 3 页 共 3 页"]
["序号","项目编码","项目名称","项目特征","计量\n单位","工程量","金额(元)",{"$nulls":4},"备注"]
[{"$nulls":6},"综合单价","合价","其中"]
[{"$nulls":8},"人工费","机械费","暂估价"]
["20",null,"PVC管","Ø25 敷设  具体要求详见招标文件","米",500,"","","","","",""]
["21",null,"开关电源","12V10A  安装 调试  具体要求详见招标文件","个",7,"","","","","",""]
["22",null,"辅材","如水晶头 端子头 接线盒等相关所有辅材","批",1]
["","","备品备件","","","","","","","",""]
[23,null,"读卡器","配置12键数字键盘K86  具体要求详见招标文件","个",2]
[null,null,"设备安装调试、管线敷设、施工监管等相关人工",null,"项",1]
[24,null,"管线敷设",null,"项",1]
[25,null,"其它相关人工",null,"项",1]
[26,null,"不停航施工费（隔离区内的的施工，投标人须采用不停航施工措施，不停航施工导致的夜间加班、工效降低、证件办理等需产生的费用必须充分考虑，费用包含在投标报价中。投标人需考虑聘请专业保安，负责门卫、巡逻、施工现场看护人数每班不得少于1人，并配备相应的保卫措施\n）",null,"项",1]
[27,null,"材料搬运及垃圾清理外运",null,"项",1]
["本页小计",{"$nulls":6},"","","","",""]
["合   计",{"$nulls":6},"","","","",""]
["分部分项工程清单与计价表"]
["专业工程名称：杭州萧山国际机场航站楼门禁系统读卡器及门禁锁改造安装工程",{"$nulls":3},"标段：",{"$nulls":4},"第 3 页 共 3 页"]
["序号","项目编码","项目名称","项目特征","计量\n单位","工程量","金额(元)",{"$nulls":4},"备注"]
[{"$nulls":6},"综合单价","合价","其中"]
[{"$nulls":8},"人工费","机械费","暂估价"]
[28,null,"措施项目",null,"项",1,"","","","","",""]
["本页小计",{"$nulls":6},"","","","",""]
["合   计",{"$nulls":6},"","","","",""]