{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["1_表1-2  分部分项工程量清单及计价表（号清单）","1_表1-3-C  技术措施项目清单及计价表"],"read":"whole","date_system":"1900"}

{"sheet":"1_表1-2  分部分项工程量清单及计价表（号清单）","index":0,"n_rows":22,"n_cols":12,"rows_kept":22,"merged":[[0,0,0,11],[1,0,1,8],[1,9,1,11],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,4,3,4],[2,5,3,5],[2,6,3,6],[2,7,3,7],[2,8,2,10],[2,11,3,11],[21,0,21,6]]}
["表 1-2 分部分项工程量清单及计价表(号清单)"]
["单位工程及专业工程名称:T4行李分拣区域增加业务配套设施-安装",{"$nulls":8},"第1页 共1页"]
["序号","项目\n编码","项目名称","项目特征描述","计量\n单位","工程量","综合单价\n(元)","合价\n(元)","其中",null,null,"备注"]
[{"$nulls":8},"人工费","机械费","管理费"]
[null,null,"[请输入分部名称,电子评标勿删]"]
[null,null,"T4行李分拣区域增加业务配套设施"]
["1","030408001001","电力电缆","4*10+1*6YJY电缆","m","245.00"]
["2","030411004001","配线","2.5平方单芯线","m","2400.00"]
["3","030411004002","配线","4平方单芯线","m","480.00"]
["4","030404019001","控制开关","3P/40A 空开","个","2"]
["5","030404019002","控制开关","3P/32A 空开","个","2"]
["6","030404019003","控制开关","2P/16A带漏保","个","10"]
["7","030404019004","控制开关","2P/20A带漏保","个","4"]
["8","030404019005","控制开关","1P/20A空开","个","2"]
["9","030411001001","配管","Dn25PVC电线管","m","400.00"]
["10","030404035001","插座","16A空调插座","个","2"]
["11","030404035002","插座","10A5孔插座","个","76"]
["12","030404017001","配电箱","32路明装电箱","台","2"]
[]
[]
[]
["合计"]

{"sheet":"1_表1-3-C  技术措施项目清单及计价表","index":1,"n_rows":22,"n_cols":12,"rows_kept":22,"merged":[[0,0,0,11],[1,0,1,8],[2,0,2,8],[2,9,2,11],[3,0,4,0],[3,1,4,1],[3,2,4,2],[3,3,4,3],[3,4,4,4],[3,5,4,5],[3,6,4,6],[3,7,4,7],[3,8,3,10],[3,11,4,11],[21,0,21,6]]}
["表1-3-C 技术措施项目清单及计价表"]
["工程名称:T4行李分拣区域增加业务配套设施"]
["单位工程及专业工程名称:T4行李分拣区域增加业务配套设施-安装",{"$nulls":8},"第1页 共1页"]
["序号","项目\n编码","项目名称","项目特征描述","计量\n单位","工程量","综合单价\n(元)","合价\n(元)","其中",null,null,"备注"]
[{"$nulls":8},"人工费","机械费","管理费"]
[null,null,"[请输入分部名称,电子评标勿删]"]
["1","03B001","脚手架搭拆费","1、由投标人综合考虑","项","1"]
["2","03B002","材料搬运及垃圾清理外运","1、由投标人综合考虑","项","1"]
["3","03B003","隔离区施工措施费\t（因隔离区内的的施工，投标人须采用相应施工措施，包括施工导致的夜间加班、工效降低、证件办理等需产生的费用必须充分考虑，费用包含在投标报价中）","1、由投标人综合考虑","项","1"]
["4","03B004","施工安全监管费\t（投标需考虑聘请专业保安（负责门卫、巡逻、施工现场看护、隔离区围界看护等工作，人数每8小时不得少于1人，并配备相应的保卫措施）","暂列金额","项","1",{"v":2000,"d":"2000.00"},{"v":2000,"d":"2000.00"}]
{"$rows_empty":11}
["合计"]